;
; FANSETUP.INF
; Copyright (c) 1999 Fancom BV, Panningen, The Netherlands
;


; Version A1.3

[version]
signature="$CHICAGO$"
Class=FNETboards
Provider=%FANCOMP%

[ClassInstall]
Addreg=ClassReg

[ClassReg]
HKR,,,,"LocalTalk and CDSnet communication adapters"
HKR,,Icon,,"-5"

[ControlFlags]
ExcludeFromSelect=PCMCIA\CDS_electronics_bv-PLT_LocalTalk_adapter-5E12

[Manufacturer]
%FANCOM%=FANCOM

[FANCOM]
%FANCOMILT%= SomePort, FANCOMILT002
%FANCOMPCNET%= PCnetPort, FANCOMPCNET001
%FANCOMPCNETPOLL%= PCnetPoll, FANCOMPCNET002
%FANCOMPCNETVIRT%= PCnetPoll, FANCOMPCNET002
%FANCOM-5E12.DeviceDesc% = PCPort,"PCMCIA\CDS_electronics_bv-PLT_LocalTalk_adapter-5E12"

; The PLT PCMCIA cards looks like a COM ports, but isn't
;-------------------------------------------------------

[PCPort]
LogConfig=caa

[SomePort]
LogConfig=c1a,c2a,c3a,c4a

[PCnetPort]
LogConfig=P200A

[PCnetPoll]
LogConfig=P200P
UpdateAutoBat=AutoBatDriver

[P200A]
ConfigPriority=HARDRECONFIG
IOConfig=200-201(3ff::), 210-211(3ff::), 300-301(3ff::), 240-241(3ff::), 204-205(3ff::), 220-221(3ff::), 310-311(3ff::)
IRQConfig=10,11

[P200P]
ConfigPriority=HARDRECONFIG
IOConfig=200-201(3ff::), 210-211(3ff::), 300-301(3ff::), 240-241(3ff::), 204-205(3ff::), 220-221(3ff::), 310-311(3ff::)

[c1a]
ConfigPriority=HARDRECONFIG
IOConfig=3f8-3ff(3ff::) 
IRQConfig=3,4,5,6,7

[c2a]
ConfigPriority=HARDRECONFIG
IOConfig=2f8-2ff(3ff::)
IRQConfig=3,4,5,6,7

[c3a]
ConfigPriority=HARDRECONFIG
IOConfig=3e8-3ef(3ff::)
IRQConfig=3,4,5,6,7

[c4a]
ConfigPriority=HARDRECONFIG
IOConfig=2e8-2ef(3ff::)
IRQConfig=3,4,5,6,7

[caa]
ConfigPriority=DESIRED
IOConfig=8@100-ffff%fff8(3ff::)
IRQConfig=3,4,5,7,9,10,11,12,13,14,15


[AutoBatDriver]
CmdAdd= SET,"FapSection=0"

[Strings]
FANCOMP="Fancom"
FANCOM="Fancom BV, Panningen, The Netherlands"
FANCOM-5E12.DeviceDesc="PLT PCMCIA LocalTalk adapter (PCnet emulation)"
FANCOMILT="ILT ISA based LocalTalk adapter (PCnet emulation)"
FANCOMPCNET="PCnet ISA based LocalTalk/CDSnet adapter (IRQ)"
FANCOMPCNETPOLL="PCnet ISA based LocalTalk/CDSnet adapter (polled mode)"
FANCOMPCNETVIRT="Virtual PCnet LocalTalk adapter for ILT/PLT/SLT"
ID1="ILT / PLT / SLT Device Driver"














